

Compex BIOS for SAMSUNG S3C4510B v1.20-lt74

Press Enter for Menu, Esc for Safe Mode

Initializing system .... Done
Found M29W800DB at 0x00000000

Loading Image From Net ................ 
bios_eth_cfg, from: 0001011c

Mini TFTP Server 1.0 (IP : 192.168.42.2)

Starting the TFTP download...

Starting the TFTP download...
..............................
Done
<4>Linux version 2.4.22-uc0 (root@codecarver) (gcc version 2.95.2 20000313 (Debian GNU/Linux)) #81 Sun Nov 2 15:24:47 CET 2003
<4>Processor: Samsung S3C4510B revision 6
<4>Architecture: SNDS100
<4>On node 0 totalpages: 2048
<4>zone(0): 0 pages.
<4>zone(1): 2048 pages.
<4>zone(2): 0 pages.
<4>Kernel command line: ip=192.168.42.2:192.168.42.1:192.168.42.1:255.255.255.0:hackme:eth0:none nfsroot=192.168.42.1:/home/p2/uclinux-arm-root
<4>Calibrating delay loop... 24.83 BogoMIPS
<6>Memory: 8MB = 8MB total
<5>Memory: 6988KB available (848K code, 175K data, 48K init)
<6>Dentry cache hash table entries: 1024 (order: 1, 8192 bytes)
<6>Inode cache hash table entries: 512 (order: 0, 4096 bytes)
<6>Mount cache hash table entries: 512 (order: 0, 4096 bytes)
<6>Buffer cache hash table entries: 1024 (order: 0, 4096 bytes)
<4>Page-cache hash table entries: 2048 (order: 1, 8192 bytes)
<4>POSIX conformance testing by UNIFIX
<6>Linux NET4.0 for Linux 2.4
<6>Based upon Swansea University Computer Society NET3.039
<4>Initializing RT netlink socket
<4>Starting kswapd
<6>Samsung S3C4510 Serial driver version 0.9 (2001-12-27) with no serial options enabled
<6>ttyS00 at 0x3ffd000 (irq = 5) is a S3C4510B
<6>ttyS01 at 0x3ffe000 (irq = 7) is a S3C4510B
<6>Samsung S3C4510 Ethernet driver version 0.1 (2002-02-20) <mac@os.nctu.edu.tw>
<6>eth0: 00:40:95:36:35:34 
<6>NET4: Linux TCP/IP 1.0 for NET4.0
<6>IP Protocols: ICMP, UDP, TCP
<6>IP: routing cache hash table of 512 buckets, 4Kbytes
<6>TCP: Hash tables configured (established 512 bind 512)
<4>IP-Config: Complete:
<4>      device=eth0, addr=192.168.42.2, mask=255.255.255.0, gw=192.168.42.1,
<4>     host=hackme, domain=, nis-domain=(none),
<4>     bootserver=192.168.42.1, rootserver=192.168.42.1, rootpath=
<4>ip_tables: (C) 2000-2002 Netfilter core team
<6>NET4: Unix domain sockets 1.0/SMP for Linux NET4.0.
<5>Looking up port of RPC 100003/2 on 192.168.42.1
<5>Looking up port of RPC 100005/1 on 192.168.42.1
<4>VFS: Mounted root (nfs filesystem).
<4>Freeing init memory: 48K
